                  DECtalk USB Jaws 4x-5x Service Pack v1.06


Access Solutions
4536 Edison Ave.
Sacramento, Ca. 95821
E-Mail: support@axsol.com
Phone: (916) 481-3559

If you plan to run the DECtalk USB as a USB device with Jaws 4.x or 5.x, do 
the following:

   1. Copy the "jsdtusb.jls" file to your Jaws 4.x-5.x directory.

   2. Edit your jfw.ini file to include the synthesizer entries 
      needed for selecting the DECtalk USB. An example of
      what your jfw.ini file should look like is included in this folder 
      for your convenience.
   
   3. Make sure the slide switch located on the right side of the unit
      is positioned towards the back of the unit.

   4. Start Jaws and select the DECtalk USB from the synthesizer
      selection menu.

