                      Window-Eyes 4.5 DECtalk USB Driver
                               (Windows 98/ME)


Access Solutions
4536 Edison Ave.
Sacramento, Ca. 95821
E-Mail: support@axsol.com
Phone: (916) 481-3559



***Important:
   Make sure you are running Window-Eyes 4.5 with service pack 4
   or later.

If you plan to run the DECtalk USB as a USB device with Window-Eyes 4.5, do 
the following:

   1. Make sure Window-Eyes is not running while you perform the
      following steps.

   2. Copy the "wedecusb.dll" file to your Wineyes directory.
   
   3. Copy the "speech32.exe" file to your Wineyes directory.

   4. Copy the "synth.ini" file to your c:\wineyes\users\default directory.

   5. Make sure the slide switch located on the right side of
      the unit is positioned towards the back of the unit.

   6. Start Window-Eyes up and select the "DECtalk USB" from the
      synthesizer selection menu.
