                 DECTALK USB QUICK INSTALLATION

                        ACCESS SOLUTIONS
                        4536 EDISON AVE.
                      SACRAMENTO, CA 95821
                       WEB: WWW.AXSOL.COM
                CUSTOMER SUPPORT: (916) 481-3559

TO INSTALL THE DECTALK USB FOLLOW THE INSTRUCTIONS LISTED BELOW.
THESE INSTRUCTIONS ARE INTENDED FOR THE MORE EXPERIENCED USER AND
NOT FOR A BEGINNER.  FOR MORE INFORMATION, REFER TO THE USERS
MANUAL (USERMAN.TXT) LOCATED ON THE DECTALK USB INSTALLATION DISK.

                    DECTALK USB INSTALLATION:

    1. MAKE SURE THE DECTALK USB IS TURNED OFF. THIS IS DONE BY
TURNING THE THUMB WHEEL COUNTER CLOCKWISE UNTIL A CLICK IS HEARD.
    2. MAKE SURE THE SLIDE SWITCH LOCATED ON THE RIGHT SIDE OF THE
UNIT IS POSITIONED TOWARDS THE BACK OF THE UNIT.  I.E AWAY FROM THE
HEADPHONE JACK OR VOLUME KNOB.
    3. BOOT YOUR COMPUTER TO A STANDARD WINDOWS DESKTOP.
    4. CONNECT THE USB CABLE, INCLUDED IN YOUR INSTALLATION KIT,
FROM THE DECTALK USB TO ONE OF THE USB PORTS LOCATED ON THE BACK OR
FRONT OF YOUR COMPUTER. KEEP IN MIND THAT SOME COMPUTERS HAVE
SEVERAL USB PORTS. ANY OF THESE PORTS WILL WORK.
    5. TURN YOUR DECTALK USB ON BY TURNING THE THUMB WHEEL
CLOCKWISE.
    6. WHEN THE ADD NEW HARDWARE WIZARD COMES UP INFORMING YOU THAT
A DECTALK USB HAS BEEN DETECTED, INSERT THE DECTALK USB
INSTALLATION CD INTO YOUR CD-ROM DRIVE AND PRESS   ENTER.
    7. WHEN PROMPTED FOR WHETHER OR NOT WINDOWS SHOULD SEARCH FOR
THE BEST DRIVER FOR THIS DEVICE, SELECT THE RADIO BUTTON THAT
ALLOWS WINDOWS TO SEARCH FOR THE BEST DRIVER FOR THIS DEVICE AND
PRESS ENTER.
    8. NEXT, CHECK THE CHECK BOX LABELED "SPECIFY A LOCATION".
    9. IN THE EDIT BOX, TYPE THE LETTER OF YOUR CD ROM DRIVE
FOLLOWED BY A COLON AND PRESS ENTER. EXAMPLE: "D:"
10. THE ADD NEW HARDWARE WIZARD WILL INFORM YOU THAT THE ACCESS
SOLUTIONS DECTALK USB HAS BEEN FOUND. JUST PRESS ENTER. IF YOU GET
A MESSAGE SAYING THAT THE SOFTWARE YOU ARE INSTALLING HAS NOT BEEN
APPROVED BY MICROSOFT, JUST PRESS THE CONTINUE BUTTON AND IGNORE
IT.
    11. ONCE YOU HAVE REACHED THIS POINT, THE ADD NEW HARDWARE
WIZARD SHOULD INFORM YOU THAT IT HAS SUCCESSFULLY INSTALLED ALL THE
NECESSARY FILES NEEDED FOR SUPPORTING YOUR NEW DECTALK USB. JUST
PRESS ENTER AND YOU ARE ALL DONE.
    12. REMOVE THE DECTALK USB INSTALLATION DISK FROM YOUR CD-ROM
DRRIVE. 
    13. UNTIL THE USB DRIVER IS READY, SELECT THE DECTALK EXPRESS
ON COMPORT XX FROM THE SYNTHESIZER SELECTION MENU FROM WITHIN YOUR
SCREEN READER. 
