
Access Solutions
4536 Edison Ave. 
Sacramento, Ca. 95821
E-Mail: support@axsol.com
Phone: (916) 481-3559

If you plan to run the Triple-Talk USB as a USB device with Jaws 3.7, do 
the following:

   1. Copy the "jsttusb.jls" file to your Jaws 3.7 directory.

   2. Edit your jfw.ini file to include the synthesizer entries 
      needed for selecting the Triple-Talk USB. An example of
      what your jfw.ini file should look like is included in this folder 
      for your convenience.

   3. Start Jaws and select the Triple-Talk USB from the synthesizer
      selection menu.

