
                          TripleTalk USB Mini Quick Installation



Access Solutions
4536 Edison Ave.
Sacramento, Ca. 95821
Web: www.axsol.com
Customer Support: (916) 481-3559



        To install the TripleTalk mini follow the instructions
listed below.  These instructions are intended for the more experienced
user and not for a beginner.  For more information, refer to 
the users manual (userman.txt) located on the TripleTalk mini
installation disk.


  TripleTalk Mini Installation:
    
    1. Boot your computer to a standard windows desktop.

    2. On one side of your TripleTalk mini you will find a volume 
       slider and a headphone jack. Move the volume slider furthest
       away from the headphone jack.
    
    3. Connect the USB cable, included in your installation kit,
       from the TripleTalk mini to an availible USB port on your 
       computer.

    4. When the Add New Hardware Wizard comes up informing you 
       that a Triple-Talk USB has been detected, insert the     
       TripleTalk mini installation disk into your CD-rom drive and press
       Enter.

    5. When prompted for whether or not windows should search for
       the best driver for this device, select the radio button that
       allows windows to search for the best driver for this device and press 
       Enter.
          
    6. Next, check the check box labeled "Specify a Location". 

    7. In the edit box, type the letter of your CD-rom drive  
       followed by a colon and press Enter.  Example: "d:"
       if you are running Vista 64bit or Windows 7 64bit
       then type "d:\tripletalk_usb_64bit"

    8. The add new hardware wizard will inform you that the Access
       Solutions Triple-Talk USB has been found. Just press Enter. If you get
A      message saying that the software you are installing has not been
       approved by Microsoft, just press the Continue button and ignore
       this message.

    9. Once you have reached this point, the add new hardware
       wizard should inform you that it has successfully installed all the 
       necessary files needed for supporting your new Triple-Talk USB. 
       Just press Enter and you are all done.
          
    10. Remove the TripleTalk mini installation disk from your CD-rom drive. 
     
    11. Select the Triple-Talk USB from the synthesizer selection 
        menu from within your screen reader. 
        
